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ANZA ELECTRIC COOPERATIVE, INC.
BOARD POLICY NO. 306
	 
INTERCONNECTION OF DISTRIBUTED GENERATION RESOURCES 

OBJECTIVE

In an effort to promote alternative types of electrical generation and subsequent interconnection with Cooperative facilities, the Cooperative has adopted this policy for the interconnection of distributed generation (DG) installations. 
This policy is adopted in accordance with Policy No. 100 – “BOARD POLICIES”.

POLICY CONTENT

The Cooperative has authorized the following categories of generation and interconnections.

A. Islanded Generation: Consumer generated energy that is in no way connected to the Cooperative’s system. Cooperative procedures, contracts or Cooperative inspections are not required for this type of installation. Local, State or Federal codes, regulations and inspections should be followed.
 
B. Net Energy Metering: Applicable to all end-use Eligible Customer-Generators who execute the applicable Net Energy Metering Interconnection Agreement (NEMIA).

An Eligible Customer-Generator is a residential, small commercial, commercial, industrial or agricultural Customer who uses a solar, wind, biogas, or fuel cell electrical generating facility, or a hybrid system of both, with a capacity of not more than 1,000 kilowatts, that is located on the Customer-Generator’s premises, is interconnected and operates in parallel with Anza Electric Cooperative Inc.’s distribution facilities, and is intended primarily to offset part or all of the Customer-Generator’s own electrical requirements on the premises.

Anza Electric Cooperative Inc. is not obligated to provide net energy metering to additional Customer-Generators when the combined total peak demand of all Customer-Generators exceeds 5 percent of the aggregate customer peak demand. 

See “Net Metering Procedures and Guidelines Manual for Members” 
EFFECTIVE DECEMBER 31, 2014, AEC HAS MET THE CALIFORNIA NEM OBLIGATION. NEM IS NO LONGER AVAILABLE FOR ANY RATE CLASS.
	
C. Interconnection of Distributed Generation (Qualifying Facilities)         Applicable to all Qualifying Facilities (QF). A QF is defined for this policy as electric generation provided by renewable energy technology installed on a retail electric member’s side of the meter. In general, this means that the DG must have as its primary energy source biomass, waste, renewable resources, geothermal resources or any combination thereof and is rated to produce an amount of electricity less than or equal to the amount of electricity the Member is reasonably expected to consume. 

D. Interconnection of Distributed Generation (DG) facilities is limited to the following:

1. For Residential Service locations, qualifying under Schedule D-1 or D-2, Domestic as an Otherwise Applicable Tariff (OAT):
a. The size of any qualifying facility, as detailed in §II(C) above, is limited in size so that the QF shall not provide more than the average monthly electric use at that location, as determined by AEC billing history for the preceding twelve (12) month period. In no case shall any DG system installed under this OAT shall exceed five (5) KW DC in nameplate rating.
2. For Commercial, Large Power, or Irrigation Service locations, qualifying under Schedule A-1, P-1, or PA-2 as an Otherwise Applicable Tariff (OAT):
a. The size of any qualifying facility, as detailed in §II(C) above, is limited in size so that the QF shall not provide more than the average monthly electric use at that location, as determined by AEC billing history for the preceding twelve (12) month period. In no case shall any DG system installed under this OAT shall exceed ten (10) KW DC in nameplate rating.

E. Each application for interconnection is subject to engineering limitations, to be determined from time-to-time. No system will be allowed to interconnect on any circuit, feeder, or other portion of the AEC system where deemed unsafe or otherwise outside the established technical limits of the affected circuit. AEC engineering is the final authority on these limitations.

F. AEC is not obligated to allow the interconnection of DG installations when the total combined output of all NEM and DG installations exceeds 10% of the historic aggregate peak demand of the entire system. 

Responsibility

The General Manager is responsible for seeing that the provisions of this policy are carried out.
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